|  |  |
| --- | --- |
| http://www.ductowire.com/images/CraneBossTitanSM.jpg(+) Larger Image | **Crane Boss® Titan Series**[« Back to Products](http://www.ductowire.com/radioRemoteControl.php)The Crane Boss TITAN Digital Radio Remote Control System comes with the following control functions:* Main Contactor/Warning Signal
* Bridge 3-5 speed reversing
* Trolley 3-5 speed reversing
* Hoist 3-5 speed reversing
* Hoist Select 1/BOTH/2 (maintained Pushbuttons with LEDs)
* Aux 3: Pushbutton (momentary)
* Aux 4: Pushbutton (momentary)
* Aux 5: Pushbutton (momentary)

Included are one portable Transmitter complete with (4) AA Batteries and Shoulder Harness; one set of Receiving equipment complete with Antenna and 15 ft. cabling; Operation & Maintenance Manual and standard Two-year Warranty.**New & Improved Features:*** Large Switches designed for use with gloves
* Strong Tactile Feedback for Speed Points
* ONLY 3-5 step Handheld on the market today
* Light, weighing in at less than 2 lbs.
* Ships in just one week!

**General Specifications:*** Operating Range: 300 feet
* Operating Temperature: -20 to 150 F
* Frequency Band: 902-918 MHz, 422-472 MHz

**Transmitter Specs:*** Housing: High-impact ABS Plastic
* (4) AA Batteries
* Internal Antenna
* LEDs for Hoist Select Pushbuttons
* Green LED for "Power ON"
* Red LED for LOW Battery & Diagnostics
* Dimensions (in inches): 4.1W x 12.0H x 2.5D
* Carry Method: Shoulder Harness
 |