|  |  |
| --- | --- |
| http://www.ductowire.com/images/CraneBossTitanSM.jpg  [(+) Larger Image](javascript:popitup('images/CraneBossTitanLG.jpg')) | **Crane Boss® Titan Series**  [« Back to Products](http://www.ductowire.com/radioRemoteControl.php)  The Crane Boss TITAN Digital Radio Remote Control System comes with the following control functions:   * Main Contactor/Warning Signal * Bridge 3-5 speed reversing * Trolley 3-5 speed reversing * Hoist 3-5 speed reversing * Hoist Select 1/BOTH/2 (maintained Pushbuttons with LEDs) * Aux 3: Pushbutton (momentary) * Aux 4: Pushbutton (momentary) * Aux 5: Pushbutton (momentary)   Included are one portable Transmitter complete with (4) AA Batteries and Shoulder Harness; one set of Receiving equipment complete with Antenna and 15 ft. cabling; Operation & Maintenance Manual and standard Two-year Warranty.  **New & Improved Features:**   * Large Switches designed for use with gloves * Strong Tactile Feedback for Speed Points * ONLY 3-5 step Handheld on the market today * Light, weighing in at less than 2 lbs. * Ships in just one week!   **General Specifications:**   * Operating Range: 300 feet * Operating Temperature: -20 to 150 F * Frequency Band: 902-918 MHz, 422-472 MHz   **Transmitter Specs:**   * Housing: High-impact ABS Plastic * (4) AA Batteries * Internal Antenna * LEDs for Hoist Select Pushbuttons * Green LED for "Power ON" * Red LED for LOW Battery & Diagnostics * Dimensions (in inches): 4.1W x 12.0H x 2.5D * Carry Method: Shoulder Harness |