**EDID Operation for the HDBaseT Transmitter:**

The EDID management map is on the bottom panel of the transmitter, and the DIP switch is just right with the map. Specific functions, please check as below:

Eg: Users want to use the internal1080P2.0 EDID,

 Pull the DIP switch D1,D 2, D3 to 010.

 Want to use the Display EDID,

 Pull the DIP switch D1,D 2,D 3 to 000.

 Want to use the External audio(3.5mm),

 Pull the DIP switch D4 to 1

Note: If need to use the internal 3.5mm audio, the video formats must be HDMI.